config

terminal

or

config(tab)

configuration terminal

or

config t

vlan vlanno.

name give\_name

exit

exit

show vlan brief

interface fastethernet 0/3

switchport mode access

switchport access vlan vlanno.

for any switch

interface fastethernet 0/3

switchport mode trunk